(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 149.0011 154.0036)
		(grid_origin 167.2844 112.4204)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "output/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3V3")
	(net 3 "Net-(ANT1-ANT)")
	(net 4 "/VBATPROT")
	(net 5 "Net-(C1-2)")
	(net 6 "Net-(C2-1)")
	(net 7 "Net-(C8-1)")
	(net 8 "/EN")
	(net 9 "/LED1")
	(net 10 "Net-(CR1-PadK)")
	(net 11 "Net-(CR2-PadK)")
	(net 12 "/NEO_PPS")
	(net 13 "Net-(CR3-PadK)")
	(net 14 "/LED2")
	(net 15 "Net-(CR4-PadK)")
	(net 16 "unconnected-(IC1-5_USB_DM-Pad5)")
	(net 17 "unconnected-(IC1-18_SDA{slash}SPI_CS_N-Pad18)")
	(net 18 "unconnected-(IC1-7_VDD_USB-Pad7)")
	(net 19 "Net-(IC1-8_RESET_N)")
	(net 20 "unconnected-(IC1-4_EXTINT-Pad4)")
	(net 21 "Net-(IC1-11_RF_IN)")
	(net 22 "unconnected-(IC1-14_LNA_EN{slash}RESERVED-Pad14)")
	(net 23 "/NEO_RX")
	(net 24 "unconnected-(IC1-6_USB_DP-Pad6)")
	(net 25 "unconnected-(IC1-2_D_SEL-Pad2)")
	(net 26 "unconnected-(IC1-17_RESERVED-Pad17)")
	(net 27 "unconnected-(IC1-1_SAFEBOOT_N-Pad1)")
	(net 28 "unconnected-(IC1-15_RESERVED-Pad15)")
	(net 29 "unconnected-(IC1-19_SCL{slash}SPI_CLK-Pad19)")
	(net 30 "unconnected-(IC1-16_RESERVED-Pad16)")
	(net 31 "/NEO_TX")
	(net 32 "/IO0")
	(net 33 "/TXD0")
	(net 34 "/RXD0")
	(net 35 "/SDA")
	(net 36 "/SCL")
	(net 37 "Net-(U7-RF_IN)")
	(net 38 "Net-(L3-2)")
	(net 39 "Net-(L3-1)")
	(net 40 "/RADIO_RST")
	(net 41 "Net-(U4-IO14)")
	(net 42 "Net-(U4-IO12)")
	(net 43 "Net-(U4-IO13)")
	(net 44 "Net-(U4-IO15)")
	(net 45 "/RADIO_MOSI")
	(net 46 "Net-(U4-IO23)")
	(net 47 "Net-(U4-IO18)")
	(net 48 "/RADIO_SCK")
	(net 49 "/RADIO_MISO")
	(net 50 "Net-(U4-IO19)")
	(net 51 "Net-(U4-IO5)")
	(net 52 "/RADIO_SS")
	(net 53 "Net-(U4-IO4)")
	(net 54 "Net-(U4-IO34)")
	(net 55 "/RADIO_BUSY")
	(net 56 "/RADIO_DIO1")
	(net 57 "Net-(U4-IO35)")
	(net 58 "Net-(U4-IO2)")
	(net 59 "/UART2RX")
	(net 60 "/UART2TX")
	(net 61 "Net-(U1-SDO{slash}ADD)")
	(net 62 "Net-(U6-FB)")
	(net 63 "/GPIO36")
	(net 64 "unconnected-(U4-SWP{slash}SD3-Pad18)")
	(net 65 "unconnected-(U4-SDO{slash}SD0-Pad21)")
	(net 66 "unconnected-(U4-IO21-Pad33)")
	(net 67 "unconnected-(U4-SHD{slash}SD2-Pad17)")
	(net 68 "unconnected-(U4-IO27-Pad12)")
	(net 69 "unconnected-(U4-SDI{slash}SD1-Pad22)")
	(net 70 "/GPIO39")
	(net 71 "unconnected-(U4-IO22-Pad36)")
	(net 72 "unconnected-(U4-SCS{slash}CMD-Pad19)")
	(net 73 "unconnected-(U4-SCK{slash}CLK-Pad20)")
	(net 74 "unconnected-(U4-IO25-Pad10)")
	(net 75 "unconnected-(U4-IO26-Pad11)")
	(net 76 "unconnected-(U5-PG-Pad3)")
	(net 77 "Net-(C12-1)")
	(net 78 "unconnected-(U5-NC-Pad7)")
	(net 79 "Net-(Q1-G)")
	(net 80 "Net-(Q1-D)")
	(net 81 "Net-(Q2-G)")
	(net 82 "Net-(U3-CS)")
	(net 83 "Net-(U5-CHG)")
	(net 84 "Net-(U5-NTC)")
	(net 85 "Net-(U5-ISET)")
	(net 86 "Net-(U5-IBF)")
	(net 87 "unconnected-(U8-DIO3-Pad11)")
	(net 88 "unconnected-(U8-NC2-Pad12)")
	(net 89 "unconnected-(U8-NC3-Pad14)")
	(net 90 "unconnected-(U8-NC-Pad7)")
	(net 91 "unconnected-(J3-D+-PadB6)")
	(net 92 "unconnected-(J3-D+-PadA6)")
	(net 93 "unconnected-(J3-D--PadA7)")
	(net 94 "unconnected-(J3-SBU1-PadA8)")
	(net 95 "unconnected-(J3-SBU2-PadB8)")
	(net 96 "unconnected-(J3-D--PadB7)")
	(net 97 "Net-(J3-CC2)")
	(net 98 "Net-(J3-CC1)")
	(net 99 "Net-(CR5-PadK)")
	(net 100 "/vbus")
	(net 101 "/vbatt-")
	(net 102 "Net-(J1-RF)")
	(net 103 "Net-(SW1-P$3)")
	(net 104 "Net-(SW1-COM)")
	(net 105 "Net-(J2-Pin_2)")
	(net 106 "Net-(J4-Pin_2)")
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 94.076 180)
		(property "Reference" "R21"
			(at -1.016 -0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(U4-IO2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.8384 113.3144 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 139.388 61.302 180)
		(property "Reference" "C9"
			(at -1.27 -0.635 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(ANT1-ANT)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 139.488 61.702) (xy 139.288 61.702) (xy 139.288 60.902) (xy 139.488 60.902)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "library_transfer:100SP1T1B1M1QEH"
		(layer "F.Cu")
		(at 177.6984 131.0894)
		(property "Reference" "SW1"
			(at -6.7056 0.7366 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Toggle Switch SPDT Panel Mount"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" thru_hole circle
			(at 0 -4.699)
			(size 3.556 3.556)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "Net-(SW1-P$3)")
			(pinfunction "P$3")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 0 4.699)
			(size 3.556 3.556)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P$2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at 0 0)
			(size 3.556 3.556)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "Net-(SW1-COM)")
			(pinfunction "COM")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 122.924 110.84 -90)
		(property "Reference" "C15"
			(at 1.778 0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 148.842 126.818 90)
		(property "Reference" "R42"
			(at -1.582 1.778 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "27k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(U6-FB)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:CC68"
		(layer "F.Cu")
		(at 160.85 104)
		(property "Reference" "U8"
			(at -6 9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.15 -7)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -7.15 -5)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 49 "/RADIO_MISO")
			(pinfunction "MISO")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -7.15 -3)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 45 "/RADIO_MOSI")
			(pinfunction "MOSI")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -7.15 -1)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 48 "/RADIO_SCK")
			(pinfunction "SCK")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -7.15 1)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 52 "/RADIO_SS")
			(pinfunction "NSS")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -7.15 3)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 40 "/RADIO_RST")
			(pinfunction "NRST")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -7.15 5)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 90 "unconnected-(U8-NC-Pad7)")
			(pinfunction "NC")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -7.15 7)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 1 "GND")
			(pinfunction "GND2")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 7.15 7)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 102 "Net-(J1-RF)")
			(pinfunction "ANT")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 7.15 5)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 1 "GND")
			(pinfunction "GND3")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 7.15 3)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 87 "unconnected-(U8-DIO3-Pad11)")
			(pinfunction "DIO3")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 7.15 1)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 88 "unconnected-(U8-NC2-Pad12)")
			(pinfunction "NC2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 7.15 -1)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 7.15 -3)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 89 "unconnected-(U8-NC3-Pad14)")
			(pinfunction "NC3")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 7.15 -5)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 56 "/RADIO_DIO1")
			(pinfunction "DIO1")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 7.15 -7)
			(size 1.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 55 "/RADIO_BUSY")
			(pinfunction "BUSY")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 173.8 102.6 90)
		(property "Reference" "C19"
			(at 1.4 0.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.45 1.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 152.198 73.094 -90)
		(property "Reference" "C2"
			(at -1.016 -0.254 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(C2-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 152.598 72.994) (xy 152.598 73.194) (xy 151.798 73.194) (xy 151.798 72.994)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 170.6 102.5 -90)
		(property "Reference" "C5"
			(at -1.016 -0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 171 102.4) (xy 171 102.6) (xy 170.2 102.6) (xy 170.2 102.4)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 121.1 70.5 90)
		(property "Reference" "R36"
			(at 1.016 0.508 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/SCL")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:S-PVSON-N10"
		(layer "F.Cu")
		(at 146.302 122.5 180)
		(property "Reference" "U6"
			(at 3.302 -2.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS63000DRCR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd roundrect
			(at -1 1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 2 "+3V3")
			(pinfunction "VOUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd roundrect
			(at -0.5 1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 38 "Net-(L3-2)")
			(pinfunction "L2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd roundrect
			(at 0 1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd roundrect
			(at 0.5 1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 39 "Net-(L3-1)")
			(pinfunction "L1")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd roundrect
			(at 1 1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 4 "/VBATPROT")
			(pinfunction "VIN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd roundrect
			(at 1 -1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 104 "Net-(SW1-COM)")
			(pinfunction "EN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd roundrect
			(at 0.5 -1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 103 "Net-(SW1-P$3)")
			(pinfunction "PS/SYNC")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "8" smd roundrect
			(at 0 -1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 103 "Net-(SW1-P$3)")
			(pinfunction "VINA")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "9" smd roundrect
			(at -0.5 -1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "10" smd roundrect
			(at -1 -1.55 270)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 62 "Net-(U6-FB)")
			(pinfunction "FB")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "PG" smd rect
			(at 0 0 270)
			(size 1.65 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "PG1" smd rect
			(at -1.55 -0.25 180)
			(size 0.7 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "PG2" smd rect
			(at -1.55 0.25 180)
			(size 0.7 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "PG3" smd rect
			(at 1.55 0.25 180)
			(size 0.7 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "PG4" smd rect
			(at 1.55 -0.25 180)
			(size 0.7 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 101.188)
		(property "Reference" "R4"
			(at 1.016 0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(U4-IO13)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/LED2")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 151.382 126.818 -90)
		(property "Reference" "R41"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "150k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(U6-FB)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 130.29 72.994)
		(property "Reference" "C16"
			(at -3.556 0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 130.19 72.594) (xy 130.39 72.594) (xy 130.39 73.394) (xy 130.19 73.394)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 120.067 77.866 90)
		(property "Reference" "R31"
			(at -3.429 0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(U1-SDO{slash}ADD)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 132.068 85.948 90)
		(property "Reference" "R10"
			(at 1.143 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "Net-(U4-IO18)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/RADIO_SCK")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603_DIODE"
		(layer "F.Cu")
		(at 143.498 104.236)
		(property "Reference" "CR1"
			(at -1.524 1.016 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at -1.27 1.778 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "A" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/LED1")
			(pinfunction "A")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "K" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(CR1-PadK)")
			(pinfunction "K")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 133.2484 113.3144 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 171.9 102.5 -90)
		(property "Reference" "C14"
			(at -3.8 0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 172.3 102.4) (xy 172.3 102.6) (xy 171.5 102.6) (xy 171.5 102.4)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 127.9 118.675 90)
		(property "Reference" "C22"
			(at -4.1594 0.624 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/vbus")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 134.608 85.948 90)
		(property "Reference" "R28"
			(at 1.143 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/UART2TX")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/NEO_RX")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 124.225 115.8 180)
		(property "Reference" "R29"
			(at -0.635 -0.635 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "Net-(J3-CC2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 131 139.5)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "AO3400A"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/vbatt-")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(Q1-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 143 121.992 -90)
		(property "Reference" "C25"
			(at 1.27 0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:MODULE_ESP32-WROOM-32D"
		(layer "F.Cu")
		(at 127.242 98.14 90)
		(property "Reference" "U4"
			(at 6.756 14.458 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ESP32-WROOM-32D-N8"
			(at -9.5 15 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(fp_text user "ANTENNA"
			(at -6 -9 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8.5 -5.26 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -8.5 -3.99 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "3V3")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at -8.5 -2.72 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/EN")
			(pinfunction "EN")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -8.5 -1.45 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/GPIO36")
			(pinfunction "SENSOR_VP")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at -8.5 -0.18 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "/GPIO39")
			(pinfunction "SENSOR_VN")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at -8.5 1.09 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(U4-IO34)")
			(pinfunction "IO34")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd rect
			(at -8.5 2.36 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(U4-IO35)")
			(pinfunction "IO35")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "8" smd rect
			(at -8.5 3.63 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "Net-(J2-Pin_2)")
			(pinfunction "IO32")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "9" smd rect
			(at -8.5 4.9 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Net-(J4-Pin_2)")
			(pinfunction "IO33")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "10" smd rect
			(at -8.5 6.17 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "unconnected-(U4-IO25-Pad10)")
			(pinfunction "IO25")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "11" smd rect
			(at -8.5 7.44 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "unconnected-(U4-IO26-Pad11)")
			(pinfunction "IO26")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "12" smd rect
			(at -8.5 8.71 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "unconnected-(U4-IO27-Pad12)")
			(pinfunction "IO27")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "13" smd rect
			(at -8.5 9.98 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(U4-IO14)")
			(pinfunction "IO14")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "14" smd rect
			(at -8.5 11.25 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(U4-IO12)")
			(pinfunction "IO12")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "15" smd rect
			(at -5.715 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "16" smd rect
			(at -4.445 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(U4-IO13)")
			(pinfunction "IO13")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "17" smd rect
			(at -3.175 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "unconnected-(U4-SHD{slash}SD2-Pad17)")
			(pinfunction "SHD/SD2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "18" smd rect
			(at -1.905 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "unconnected-(U4-SWP{slash}SD3-Pad18)")
			(pinfunction "SWP/SD3")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "19" smd rect
			(at -0.635 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "unconnected-(U4-SCS{slash}CMD-Pad19)")
			(pinfunction "SCS/CMD")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "20" smd rect
			(at 0.635 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(U4-SCK{slash}CLK-Pad20)")
			(pinfunction "SCK/CLK")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "21" smd rect
			(at 1.905 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(U4-SDO{slash}SD0-Pad21)")
			(pinfunction "SDO/SD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "22" smd rect
			(at 3.175 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "unconnected-(U4-SDI{slash}SD1-Pad22)")
			(pinfunction "SDI/SD1")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "23" smd rect
			(at 4.445 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U4-IO15)")
			(pinfunction "IO15")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "24" smd rect
			(at 5.715 12.25 90)
			(size 0.9 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(U4-IO2)")
			(pinfunction "IO2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "25" smd rect
			(at 8.5 11.25 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/IO0")
			(pinfunction "IO0")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "26" smd rect
			(at 8.5 9.98 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "Net-(U4-IO4)")
			(pinfunction "IO4")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "27" smd rect
			(at 8.5 8.71 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/UART2RX")
			(pinfunction "IO16")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "28" smd rect
			(at 8.5 7.44 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/UART2TX")
			(pinfunction "IO17")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "29" smd rect
			(at 8.5 6.17 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(U4-IO5)")
			(pinfunction "IO5")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "30" smd rect
			(at 8.5 4.9 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "Net-(U4-IO18)")
			(pinfunction "IO18")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "31" smd rect
			(at 8.5 3.63 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "Net-(U4-IO19)")
			(pinfunction "IO19")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "32" smd rect
			(at 8.5 2.36 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "33" smd rect
			(at 8.5 1.09 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "unconnected-(U4-IO21-Pad33)")
			(pinfunction "IO21")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "34" smd rect
			(at 8.5 -0.18 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "/RXD0")
			(pinfunction "RXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "35" smd rect
			(at 8.5 -1.45 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/TXD0")
			(pinfunction "TXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "36" smd rect
			(at 8.5 -2.72 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "unconnected-(U4-IO22-Pad36)")
			(pinfunction "IO22")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "37" smd rect
			(at 8.5 -3.99 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U4-IO23)")
			(pinfunction "IO23")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "38" smd rect
			(at 8.5 -5.26 90)
			(size 2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_1" smd rect
			(at -2.835 0.405 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_2" smd rect
			(at -1 0.405 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_3" smd rect
			(at 0.835 0.405 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_4" smd rect
			(at -2.835 2.24 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_5" smd rect
			(at -1 2.24 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_6" smd rect
			(at 0.835 2.24 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_7" smd rect
			(at -2.835 4.075 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_8" smd rect
			(at -1 4.075 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "39_9" smd rect
			(at 0.835 4.075 90)
			(size 1.33 1.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 120.792 107.14) (xy 120.792 89.14) (xy 114.492 89.14) (xy 114.492 107.14)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 120.792 107.14) (xy 120.792 89.14) (xy 114.492 89.14) (xy 114.492 107.14)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:SHT40"
		(layer "F.Cu")
		(at 118.924 70.5 90)
		(property "Reference" "U2"
			(at 1.3 -0.124 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SHT40-AD1B-R2"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.7 -0.4 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -0.7 0.4 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 0.7 0.4 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 0.7 -0.4 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 133.338 85.948 90)
		(property "Reference" "R12"
			(at 1.143 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(U4-IO5)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "/RADIO_SS")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 125.275 118.675 90)
		(property "Reference" "C23"
			(at -1.3654 -0.4086 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/vbus")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603_DIODE"
		(layer "F.Cu")
		(at 165.914 87.318 90)
		(property "Reference" "CR2"
			(at -1.27 -0.762 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "A" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "A")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "K" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(CR2-PadK)")
			(pinfunction "K")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 135.878 85.948 90)
		(property "Reference" "R27"
			(at 1.143 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/UART2RX")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/NEO_TX")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 133 135.5 -90)
		(property "Reference" "R22"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "Net-(U3-CS)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 146.302 126.818 -90)
		(property "Reference" "C24"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "Net-(SW1-P$3)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 152.144 121.992 -90)
		(property "Reference" "C30"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 118.797 77.866 90)
		(property "Reference" "C6"
			(at -2.413 0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 118.397 77.966) (xy 118.397 77.766) (xy 119.197 77.766) (xy 119.197 77.966)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603_DIODE"
		(layer "F.Cu")
		(at 124.65 125.01695 -90)
		(property "Reference" "CR5"
			(at 1.68305 0.55 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "A" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/vbus")
			(pinfunction "A")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "K" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "Net-(CR5-PadK)")
			(pinfunction "K")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 123.178 85.948 90)
		(property "Reference" "R9"
			(at -0.635 1.651 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U4-IO23)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/RADIO_MOSI")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 161.85 92.144 90)
		(property "Reference" "C4"
			(at -0.635 1.524 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 161.45 92.244) (xy 161.45 92.044) (xy 162.25 92.044) (xy 162.25 92.244)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "library_transfer:SMA_SMD_VERT"
		(layer "F.Cu")
		(at 168.0972 117.7036)
		(property "Reference" "J1"
			(at -5.6388 0.3048 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMA Connector Jack, Female Socket 50Ohm Surface Mount Solder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "DND4" smd rect
			(at 2.75 2.75)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "GND1" smd rect
			(at -2.75 -2.75)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" smd rect
			(at 2.75 -2.75)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" smd rect
			(at -2.75 2.75)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "SIG" smd roundrect
			(at 0 0)
			(size 1.55 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.5)
			(net 102 "Net-(J1-RF)")
			(pinfunction "RF")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 144.174 71.786 90)
		(property "Reference" "C8"
			(at -1.016 -0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22nF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(C8-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 143.774 71.886) (xy 143.774 71.686) (xy 144.574 71.686) (xy 144.574 71.886)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 165.914 78.428 90)
		(property "Reference" "R7"
			(at -0.635 -0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(CR3-PadK)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 136 128.5 180)
		(property "Reference" "R19"
			(at -1.4 -0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at -1.27 1.778 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 180)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 180)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(C12-1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 136.5 125 -90)
		(property "Reference" "R25"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "Net-(U5-ISET)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 126.734 110.586 90)
		(property "Reference" "C11"
			(at -1.27 -0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/EN")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 126.334 110.686) (xy 126.334 110.486) (xy 127.134 110.486) (xy 127.134 110.686)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 147.6 108.1 -90)
		(property "Reference" "R20"
			(at -1.143 1.651 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/RADIO_RST")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:6DFN-1X1.6"
		(layer "F.Cu")
		(at 144.428 69.5 -90)
		(property "Reference" "U7"
			(at 1.286 1.028 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AT2659"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.45 -0.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -0.5 0)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at -0.5 0.5)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(U7-RF_IN)")
			(pinfunction "RF_IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 0.5 0.5)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(C8-1)")
			(pinfunction "VS")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at 0.5 0)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(C8-1)")
			(pinfunction "EN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 0.5 -0.5)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(IC1-11_RF_IN)")
			(pinfunction "RF_OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:10DFN"
		(layer "F.Cu")
		(at 131.5 121.5)
		(property "Reference" "U5"
			(at -2.032 -2.032 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LP28013A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -1.65 -1)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/vbus")
			(pinfunction "VIN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -1.65 -0.5)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "Net-(U5-CHG)")
			(pinfunction "CHG")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at -1.65 0)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "unconnected-(U5-PG-Pad3)")
			(pinfunction "PG")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -1.65 0.5)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "EN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at -1.65 1)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "Net-(U5-NTC)")
			(pinfunction "NTC")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 1.65 1)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd rect
			(at 1.65 0.5)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(U5-NC-Pad7)")
			(pinfunction "NC")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "8" smd rect
			(at 1.65 0)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U5-IBF)")
			(pinfunction "IBF")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "9" smd rect
			(at 1.65 -0.5)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "Net-(U5-ISET)")
			(pinfunction "ISET")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "10" smd rect
			(at 1.65 -1)
			(size 0.8 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "BAT")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "GF" smd rect
			(at 0 0 90)
			(size 2.4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 146.304 133.5532 -90)
		(property "Reference" "C27"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "Net-(SW1-COM)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:1X06_325"
		(layer "F.Cu")
		(at 129.274 80.106 180)
		(descr "PIN HEADER")
		(property "Reference" "JP1"
			(at 6.8072 -1.7018 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PINHD-1X6"
			(at -7.62 3.175 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" thru_hole oval
			(at -6.35 0 270)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole oval
			(at -3.81 0 270)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/IO0")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole oval
			(at -1.27 0 270)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/EN")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole oval
			(at 1.27 0 270)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/RXD0")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole oval
			(at 3.81 0 270)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/TXD0")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole oval
			(at 6.35 0 270)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 124.956 110.84 -90)
		(property "Reference" "C20"
			(at 1.778 0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/EN")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 117.4 70.5 -90)
		(property "Reference" "C7"
			(at 0.889 0.762 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 117.8 70.4) (xy 117.8 70.6) (xy 117 70.6) (xy 117 70.4)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:NEO-M8"
		(layer "F.Cu")
		(at 155.5 83 90)
		(descr "u-blox NEO GNSS module")
		(property "Reference" "IC1"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NEO-M8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(fp_text user "u-blox NEO"
			(at 4.29 -0.9 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at 6.4 7.4 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(IC1-1_SAFEBOOT_N-Pad1)")
			(pinfunction "1_SAFEBOOT_N")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 6.4 6.3 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(IC1-2_D_SEL-Pad2)")
			(pinfunction "2_D_SEL")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 6.4 5.2 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/NEO_PPS")
			(pinfunction "3_TIMEPULSE")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 6.4 4.1 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(IC1-4_EXTINT-Pad4)")
			(pinfunction "4_EXTINT")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at 6.4 3 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(IC1-5_USB_DM-Pad5)")
			(pinfunction "5_USB_DM")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 6.4 1.9 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(IC1-6_USB_DP-Pad6)")
			(pinfunction "6_USB_DP")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd rect
			(at 6.4 0.8 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(IC1-7_VDD_USB-Pad7)")
			(pinfunction "7_VDD_USB")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "8" smd rect
			(at 6.4 -2.2 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(IC1-8_RESET_N)")
			(pinfunction "8_RESET_N")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "9" smd rect
			(at 6.4 -3.3 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(C2-1)")
			(pinfunction "9_VCC_RF")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "10" smd rect
			(at 6.4 -4.4 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "10_GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "11" smd rect
			(at 6.4 -5.5 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(IC1-11_RF_IN)")
			(pinfunction "11_RF_IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "12" smd rect
			(at 6.4 -6.6 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "12_GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "13" smd rect
			(at -5.6 -6.6 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "13_GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "14" smd rect
			(at -5.6 -5.5 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(IC1-14_LNA_EN{slash}RESERVED-Pad14)")
			(pinfunction "14_LNA_EN/RESERVED")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "15" smd rect
			(at -5.6 -4.4 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(IC1-15_RESERVED-Pad15)")
			(pinfunction "15_RESERVED")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "16" smd rect
			(at -5.6 -3.3 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(IC1-16_RESERVED-Pad16)")
			(pinfunction "16_RESERVED")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "17" smd rect
			(at -5.6 -2.2 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(IC1-17_RESERVED-Pad17)")
			(pinfunction "17_RESERVED")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "18" smd rect
			(at -5.6 0.8 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(IC1-18_SDA{slash}SPI_CS_N-Pad18)")
			(pinfunction "18_SDA/SPI_CS_N")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "19" smd rect
			(at -5.6 1.9 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(IC1-19_SCL{slash}SPI_CLK-Pad19)")
			(pinfunction "19_SCL/SPI_CLK")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "20" smd rect
			(at -5.6 3 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/NEO_TX")
			(pinfunction "20_TXD/SPI_MISO")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "21" smd rect
			(at -5.6 4.1 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/NEO_RX")
			(pinfunction "21_RXD/SPI_MOSI")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "22" smd rect
			(at -5.6 5.2 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "22_V_BCKP")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "23" smd rect
			(at -5.6 6.3 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "23_VCC")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "24" smd rect
			(at -5.6 7.4 180)
			(size 0.8 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "24_GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 135.5 139.5 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "AO3400A"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Net-(Q2-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(Q1-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 143.762 126.818 -90)
		(property "Reference" "R43"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "Net-(SW1-P$3)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603_DIODE"
		(layer "F.Cu")
		(at 143.498 99.41)
		(property "Reference" "CR4"
			(at -1.524 1.016 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at -1.27 1.778 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "A" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/LED2")
			(pinfunction "A")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "K" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(CR4-PadK)")
			(pinfunction "K")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 153.468 73.094 -90)
		(property "Reference" "R18"
			(at -3.794 0.568 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(IC1-8_RESET_N)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 134.29 125 -90)
		(property "Reference" "R26"
			(at -1.27 2.09 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U5-IBF)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 140.658 65.874 135)
		(property "Reference" "C1"
			(at -0.762004 -0.508001 135)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.499999 0 315)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(ANT1-ANT)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.499999 0 315)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(C1-2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 140.445868 66.227553) (xy 140.304447 66.086132) (xy 140.870132 65.520447) (xy 141.011553 65.661868)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 95.346)
		(property "Reference" "R5"
			(at 1.016 0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U4-IO15)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/SCL")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 129.274 110.586 90)
		(property "Reference" "R15"
			(at -1.143 -0.381 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/RADIO_BUSY")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(U4-IO34)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 140.46 118.69 90)
		(property "Reference" "C21"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 132.5 129)
		(property "Reference" "C12"
			(at -1.5 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.499999 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(C12-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.499999 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "/vbatt-")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 132.4 128.6) (xy 132.6 128.6) (xy 132.6 129.4) (xy 132.4 129.4)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 128.004 110.586 -90)
		(property "Reference" "R8"
			(at 1.143 0.381 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/EN")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 106.014)
		(property "Reference" "R3"
			(at 1.016 0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(U4-IO12)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/LED1")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 117.273 77.866 90)
		(property "Reference" "C13"
			(at -3.429 0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 116.873 77.966) (xy 116.873 77.766) (xy 117.673 77.766) (xy 117.673 77.966)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:CY43"
		(layer "F.Cu")
		(at 146.302 117.166 180)
		(property "Reference" "L3"
			(at -2.698 -0.434 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 1.625 0 270)
			(size 4.5 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(L3-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -1.625 0 270)
			(size 4.5 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "Net-(L3-2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 121.6 75.1 -90)
		(property "Reference" "R35"
			(at -1.5 -0.6 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/SDA")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 130.544 110.586 90)
		(property "Reference" "R16"
			(at -1.143 -0.381 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/RADIO_DIO1")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(U4-IO35)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.65 71.786 90)
		(property "Reference" "R1"
			(at -1.143 -0.381 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(C2-1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(C8-1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 160.1978 127.4046 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at -3.8082 0.0706 90)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 129 125 -90)
		(property "Reference" "R24"
			(at 1.5 0.6 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "Net-(U5-NTC)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 166.8978 127.4046 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at -3.8082 0.0706 90)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 107.538)
		(property "Reference" "R2"
			(at 1.016 0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(U4-IO14)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/RADIO_RST")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 132.576 72.994 180)
		(property "Reference" "R17"
			(at 1.376 0.694 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/IO0")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 137.148 85.948 90)
		(property "Reference" "R13"
			(at 1.143 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "Net-(U4-IO4)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/SDA")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 160.58 92.144 90)
		(property "Reference" "C3"
			(at -0.635 -0.508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 160.18 92.244) (xy 160.18 92.044) (xy 160.98 92.044) (xy 160.98 92.244)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 157.278 92.017 180)
		(property "Reference" "C17"
			(at -1.27 -0.762 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 180)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 180)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0402_INDUCTOR"
		(layer "F.Cu")
		(at 142.396 67.468 135)
		(property "Reference" "L1"
			(at -0.762004 -0.508001 135)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "6.8nH"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at 0.499999 0 315)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(C1-2)")
			(pinfunction "P$1")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at -0.499999 0 315)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(U7-RF_IN)")
			(pinfunction "P$2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 142.183868 67.821553) (xy 142.042447 67.680132) (xy 142.608132 67.114447) (xy 142.749553 67.255868)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 149.604 121.992 -90)
		(property "Reference" "C29"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:W3010"
		(layer "F.Cu")
		(at 146.5 58 180)
		(property "Reference" "ANT1"
			(at -2.286 -1.778 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "W3010"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "P$1" smd rect
			(at -4.55 0 180)
			(size 1.7 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" smd rect
			(at 4.55 -0.875 180)
			(size 1.7 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(ANT1-ANT)")
			(pinfunction "ANT")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "P$3" smd rect
			(at 4.55 0.875 180)
			(size 1.7 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 151.9 59.75) (xy 151.9 62.25) (xy 141.1 62.25) (xy 141.1 59.75) (xy 143 59.75) (xy 143 56.25)
					(xy 141.1 56.25) (xy 141.1 56) (xy 151.9 56) (xy 151.9 56.25) (xy 150 56.25) (xy 150 59.75)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 151.9 59.75) (xy 151.9 62.25) (xy 141.1 62.25) (xy 141.1 59.75) (xy 141.1 56.25) (xy 141.1 56)
					(xy 151.9 56) (xy 151.9 56.25)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 97.632)
		(property "Reference" "R14"
			(at -1.27 -0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(CR4-PadK)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 146.304 130.2004 -90)
		(property "Reference" "R33"
			(at -1.27 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "150k"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "Net-(SW1-COM)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 119.35 127.3 180)
		(property "Reference" "R30"
			(at -0.635 -0.635 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 180)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "Net-(J3-CC1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "library_transfer:SOT23-6"
		(layer "F.Cu")
		(at 133 132)
		(property "Reference" "U3"
			(at 1.7 0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1.75 2 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SOT-23-6 Battery Protection UVLO, OV, OC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(fp_text user "*"
			(at -1.75 1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at -0.95 1.15 90)
			(size 0.9 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "Net-(Q1-G)")
			(pinfunction "OD")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0 1.15 90)
			(size 0.9 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "Net-(U3-CS)")
			(pinfunction "CS")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 0.95 1.15 90)
			(size 0.9 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "Net-(Q2-G)")
			(pinfunction "OC")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 0.95 -1.15 90)
			(size 0.9 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at 0 -1.15 90)
			(size 0.9 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(C12-1)")
			(pinfunction "VDD")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at -0.95 -1.15 90)
			(size 0.9 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "/vbatt-")
			(pinfunction "VSS")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 170.2478 127.4046 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -3.8082 0.0706 90)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 140.46 121.992 -90)
		(property "Reference" "C26"
			(at 1.27 0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 163.5478 127.4046 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at -3.8082 0.0706 90)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 137.92 118.69 90)
		(property "Reference" "C10"
			(at -1.27 -1.118 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:BME280"
		(layer "F.Cu")
		(at 118.289 74.818)
		(property "Reference" "U1"
			(at 2.54 0.762 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BMP280"
			(at -1.27 1.524 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.975 -0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND1")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -0.325 -0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "CSB")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 0.325 -0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/SDA")
			(pinfunction "SDI/SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 0.975 -0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/SCL")
			(pinfunction "SCK/SCL")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at 0.975 0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(U1-SDO{slash}ADD)")
			(pinfunction "SDO/ADD")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 0.325 0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "VDDIO")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd rect
			(at -0.325 0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "8" smd rect
			(at -0.975 0.9 90)
			(size 0.7 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "library_transfer:MC-118LD-H65"
		(layer "F.Cu")
		(at 119.325 120.05 90)
		(property "Reference" "J3"
			(at -0.0254 3.302 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USB_C_Receptacle_pwr_usb2"
			(at -1.9794 8.462 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.05 -2.325 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" thru_hole circle
			(at -3.85 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" thru_hole circle
			(at -2.75 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/vbus")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" thru_hole circle
			(at -1.65 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "Net-(J3-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" thru_hole circle
			(at -0.55 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(J3-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" thru_hole circle
			(at 0.55 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(J3-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" thru_hole circle
			(at 1.65 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(J3-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional")
		)
		(pad "A9" thru_hole circle
			(at 2.75 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/vbus")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" thru_hole circle
			(at 3.85 -0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" thru_hole circle
			(at 3.85 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" thru_hole circle
			(at 2.75 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/vbus")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" thru_hole circle
			(at 1.65 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "Net-(J3-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" thru_hole circle
			(at 0.55 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(J3-D+-PadB6)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" thru_hole circle
			(at -0.55 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "unconnected-(J3-D--PadB7)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" thru_hole circle
			(at -1.65 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(J3-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional")
		)
		(pad "B9" thru_hole circle
			(at -2.75 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/vbus")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" thru_hole circle
			(at -3.85 0.675 90)
			(size 0.95 0.95)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -2.5 -2.15 90)
			(size 1.6 0.9)
			(drill oval 1.3 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "S1" thru_hole oval
			(at -2.5 2.15 90)
			(size 1.6 0.9)
			(drill oval 1.3 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "S1" thru_hole oval
			(at 2.5 -2.15 90)
			(size 1.6 0.9)
			(drill oval 1.3 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "S1" thru_hole oval
			(at 2.5 2.15 90)
			(size 1.6 0.9)
			(drill oval 1.3 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 165.914 84.016 -90)
		(property "Reference" "R6"
			(at 0.635 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 270)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(CR2-PadK)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 126.84 125 90)
		(property "Reference" "R23"
			(at -1.4 -0.64 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "Net-(CR5-PadK)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "Net-(U5-CHG)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603"
		(layer "F.Cu")
		(at 135.325 118.675 90)
		(property "Reference" "C18"
			(at 1.475 -1.925 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 142.99 102.458)
		(property "Reference" "R32"
			(at 1.016 0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(CR1-PadK)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:R0402"
		(layer "F.Cu")
		(at 130.798 85.948 90)
		(property "Reference" "R11"
			(at 1.143 0.635 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "1" smd rect
			(at -0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "Net-(U4-IO19)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.5 0 90)
			(size 0.6 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "/RADIO_MISO")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:0603_DIODE"
		(layer "F.Cu")
		(at 165.914 75.126 -90)
		(property "Reference" "CR3"
			(at -1.016 1.778 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at -1.27 1.778 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(pad "A" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/NEO_PPS")
			(pinfunction "A")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "K" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(CR3-PadK)")
			(pinfunction "K")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:18650"
		(layer "B.Cu")
		(at 133 104.5 90)
		(property "Reference" "B1"
			(at -38.1 11.43 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BH-18650-B1BA002"
			(at 9.424 -4.395 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(fp_text user "_"
			(at -42.8 9.2 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "+"
			(at 41 9 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 35.84 -8 90)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "+" smd rect
			(at 39.63 0 90)
			(size 8 7.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "+")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "-" smd rect
			(at -39.63 0 90)
			(size 8 7.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 101 "/vbatt-")
			(pinfunction "-")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "meshtastic_base_rbrd:18650"
		(layer "B.Cu")
		(at 164.6571 104.6016 90)
		(property "Reference" "B2"
			(at -37.2574 10.5775 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BH-18650-B1BA002"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "meshtastic_base_rbrd.kicad_sch")
		(fp_text user "+"
			(at 41 4 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "_"
			(at -42.2984 5.7429 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 35.84 -8 90)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "+" smd rect
			(at 39.63 0 90)
			(size 8 7.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/VBATPROT")
			(pinfunction "+")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(pad "-" smd rect
			(at -39.63 0 90)
			(size 8 7.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 101 "/vbatt-")
			(pinfunction "-")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(solder_paste_margin 0)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 170.5011 153.035)
		(mid 173.955158 143.696165)
		(end 183.0011 139.535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.0011 68.5036)
		(end 183.0011 139.535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.5011 56.0036)
		(end 170.5011 56.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.5011 153.035)
		(end 127.5011 153.035)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114.0011 139.535)
		(mid 123.547042 143.489058)
		(end 127.5011 153.035)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 183.0011 68.5036)
		(mid 174.162265 64.842435)
		(end 170.5011 56.0036)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127.5011 56.0036)
		(mid 123.339935 65.049542)
		(end 114.0011 68.5036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.0011 139.535)
		(end 114.0011 68.5036)
		(layer "Edge.Cuts")
	)
	(gr_text "007\n"
		(at 180.820168 81.821003 270)
		(layer "B.Mask")
	)
	(gr_text "GND"
		(at 135.624 78.074 90)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 125.464 78.074 90)
		(layer "F.SilkS")
	)
	(gr_text "PWR"
		(at 167.692 86.556 90)
		(layer "F.SilkS")
	)
	(gr_text "LOCK\n"
		(at 148.5392 99.5172 0)
		(layer "F.SilkS")
	)
	(gr_text "V"
		(at 122.924 78.074 90)
		(layer "F.SilkS")
	)
	(gr_text "IO0"
		(at 133.084 78.074 90)
		(layer "F.SilkS")
	)
	(gr_text "EN"
		(at 130.544 78.074 90)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 146.812 104.2924 0)
		(layer "F.SilkS")
	)
	(gr_text "PPS"
		(at 167.692 75.126 90)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 128.004 78.074 90)
		(layer "F.SilkS")
	)
	(gr_text "Tracker / Repeater\n"
		(at 176.632268 84.530203 270)
		(layer "B.SilkS")
	)
	(gr_text "MMXXVI\n"
		(at 179.150368 76.093303 270)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 163.9824 113.6904) (xy 172.1104 113.6904) (xy 172.1104 121.8184) (xy 163.9824 121.8184)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/VBATPROT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.8358 118.9948) (xy 141.126563 118.9948) (xy 142.142564 120.0108) (xy 145.190563 120.0108)
				(xy 145.4892 120.309437) (xy 145.4892 121.5602) (xy 144.428564 121.5602) (xy 144.301563 121.6872)
				(xy 132.8358 121.6872)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.5732 107.8484) (xy 169.3672 107.8484) (xy 169.3672 110.0836) (xy 166.5732 110.0836)
			)
		)
	)
	(zone
		(net 100)
		(net_name "/vbus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.25 120.625) (xy 130.25 120.375) (xy 129.45 120.375) (xy 128.4 119.325) (xy 128.4 118.975)
				(xy 124.775 118.975) (xy 122.025 116.225) (xy 122.025 116.175) (xy 120.7 116.175) (xy 120.05 116.825)
				(xy 118.625 116.825) (xy 118.625 123.275) (xy 120.075 123.275) (xy 120.7 123.9) (xy 122.05 123.9)
				(xy 125.875 120.075) (xy 128.4 120.075) (xy 128.95 120.625)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.175436 121.5602) (xy 147.1148 121.5602) (xy 147.1148 120.309437) (xy 147.413437 120.0108)
				(xy 153.9982 120.0108) (xy 153.9982 121.6872) (xy 148.302437 121.6872)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.7662 56.3998) (xy 142.7662 57.8222) (xy 140.9882 57.8222) (xy 140.9882 58.3302) (xy 140.3278 58.3302)
				(xy 140.3278 56.3998)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.1)
		)
		(min_thickness 0.09525)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2405)
			(thermal_bridge_width 0.2405)
		)
		(polygon
			(pts
				(xy 182 56.125) (xy 182 139.5) (xy 115 139.5) (xy 115 56.125)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.6722 56.3998) (xy 152.6722 60.1082) (xy 150.2338 60.1082) (xy 150.2338 56.3998)
			)
		)
	)
	(zone
		(net 101)
		(net_name "/vbatt-")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169 140) (xy 169 149) (xy 128 149) (xy 128 140)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.09525)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.2405)
			(thermal_bridge_width 0.2405)
		)
		(polygon
			(pts
				(arc
					(start 167.0812 117.7036)
					(mid 169.1132 117.7036)
					(end 167.0812 117.7036)
				)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.SilkS")
		(name "obstruct")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.3 113.3) (xy 150 113.3) (xy 150.5 113.3) (xy 150.5 119.9) (xy 147.7 119.9) (xy 146.9 119.1)
				(xy 145.7 119.1) (xy 144.9 119.9) (xy 142.3 119.9)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.09525)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.2405)
			(thermal_bridge_width 0.2405)
		)
		(polygon
			(pts
				(xy 166.7002 110.0836) (xy 169.3672 110.0836) (xy 169.3672 112.1156) (xy 166.7002 112.1156)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2024)
			(thermal_bridge_width 0.2024)
		)
		(polygon
			(pts
				(xy 182 56.1) (xy 182 69.5) (xy 182 139.5) (xy 115 139.5) (xy 115 56.1)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 179.005658 79.516424) (xy 178.972145 79.58453) (xy 178.962172 79.758078) (xy 178.971207 79.948816)
				(xy 179.016051 80.091313) (xy 179.078898 80.205038) (xy 179.191961 80.344115) (xy 179.326953 80.443109)
				(xy 179.462437 80.511354) (xy 179.602329 80.560668) (xy 179.752311 80.597913) (xy 179.869489 80.610931)
				(xy 180.046356 80.606891) (xy 180.164373 80.601845) (xy 180.308755 80.579786) (xy 180.422283 80.538595)
				(xy 180.55324 80.488226) (xy 180.666369 80.42115) (xy 180.757116 80.348555) (xy 180.828801 80.290807)
				(xy 180.900299 80.187531) (xy 180.97237 80.033384) (xy 180.995245 79.922979) (xy 181.003283 79.782318)
				(xy 180.99928 79.692226) (xy 180.984959 79.600165) (xy 180.990282 79.50013) (xy 181.302854 78.989387)
				(xy 181.309861 78.993676) (xy 181.316167 78.990901) (xy 181.394486 79.168893) (xy 181.463002 79.339673)
				(xy 181.5 79.5) (xy 181.509275 79.60718) (xy 181.505186 79.925162) (xy 181.463195 80.105422) (xy 181.426302 80.252982)
				(xy 181.370786 80.37327) (xy 181.296842 80.511911) (xy 181.181492 80.64992) (xy 181.001237 80.8015)
				(xy 180.844338 80.904047) (xy 180.650867 80.992082) (xy 180.42586 81.068788) (xy 180.240653 81.102555)
				(xy 180.052571 81.125044) (xy 179.867902 81.125044) (xy 179.618188 81.084107) (xy 179.352707 81.005484)
				(xy 179.190801 80.940925) (xy 179.039285 80.853905) (xy 178.872969 80.743029) (xy 178.729121 80.580687)
				(xy 178.618316 80.41961) (xy 178.525971 80.216444) (xy 178.467414 79.994549) (xy 178.46126 79.791484)
				(xy 178.470458 79.560498) (xy 178.49816 79.412751) (xy 178.540079 79.261435) (xy 178.608677 79.067927)
				(xy 178.661321 78.975476)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 179.657099 78.147134) (xy 179.61999 78.300731) (xy 179.546055 78.498913) (xy 179.47233 78.609504)
				(xy 179.362458 78.802098) (xy 179.362458 78.752377) (xy 179.090747 78.255935) (xy 179.125223 78.178359)
				(xy 179.137945 78.112798) (xy 179.143005 77.830547) (xy 179.143005 76.318347) (xy 179.657099 76.318347)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 180.809243 77.797993) (xy 180.818329 78.134223) (xy 180.840536 78.199875) (xy 180.871266 78.245404)
				(xy 180.602545 78.755051) (xy 180.592314 78.749658) (xy 180.588333 78.75563) (xy 180.558493 78.735739)
				(xy 180.488722 78.618064) (xy 180.391943 78.425524) (xy 180.341409 78.319297) (xy 180.326643 78.243367)
				(xy 180.326643 70.699866) (xy 180.809243 70.699866)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.SilkS")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 179.306665 81.096452) (xy 179.437629 81.141788) (xy 179.591532 81.177999) (xy 179.66218 81.183988)
				(xy 179.66218 84.306141) (xy 179.147068 84.306141) (xy 179.147068 81.040716) (xy 179.159585 81.040716)
				(xy 179.166085 81.03421)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.SilkS")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 179.053622 77.614679) (xy 179.02956 77.644207) (xy 178.998236 77.719579) (xy 178.980318 77.809172)
				(xy 178.962223 77.990123) (xy 178.980252 78.156392) (xy 179.025535 78.31538) (xy 179.085024 78.473682)
				(xy 179.1799 78.655359) (xy 179.435805 79.053433) (xy 179.546043 79.24635) (xy 179.634282 79.449501)
				(xy 179.657099 79.575005) (xy 179.657099 80.48463) (xy 179.633844 80.461382) (xy 179.525986 80.434413)
				(xy 179.405496 80.369536) (xy 179.279322 80.295072) (xy 179.204589 80.201657) (xy 179.147068 80.124961)
				(xy 179.147068 79.624666) (xy 179.129593 79.563504) (xy 179.075437 79.455196) (xy 179.011801 79.346101)
				(xy 178.828894 79.066661) (xy 178.700484 78.842454) (xy 178.567834 78.571033) (xy 178.494125 78.345807)
				(xy 178.457205 78.133512) (xy 178.457205 77.852108) (xy 178.479762 77.695216) (xy 178.525897 77.497359)
				(xy 178.595822 77.344137) (xy 178.688113 77.192375) (xy 178.775691 77.085217) (xy 178.937679 76.942712)
				(xy 179.049397 76.869469)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.SilkS")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 180.205739 76.625402) (xy 180.205739 77.141538) (xy 180.105288 77.124992) (xy 180.033183 77.120988)
				(xy 179.937237 77.120988) (xy 179.819504 77.125012) (xy 179.755813 77.13671) (xy 179.750505 76.635807)
				(xy 179.781786 76.611328) (xy 179.845021 76.605875) (xy 180.01589 76.605875)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.SilkS")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 180.977399 76.900545) (xy 181.158073 77.057608) (xy 181.291691 77.209726) (xy 181.407582 77.427152)
				(xy 181.490803 77.649071) (xy 181.513337 77.938971) (xy 181.509243 78.229759) (xy 181.42623 78.524915)
				(xy 181.310703 78.777439) (xy 181.110068 79.107416) (xy 180.958842 79.340853) (xy 180.823443 79.588583)
				(xy 180.819379 80.128353) (xy 180.789357 80.178388) (xy 180.700402 80.267342) (xy 180.603578 80.345625)
				(xy 180.464477 80.424963) (xy 180.342469 80.466675) (xy 180.318458 80.466675) (xy 180.322585 79.525287)
				(xy 180.34127 79.413177) (xy 180.382719 79.31059) (xy 180.502232 79.094036) (xy 180.744927 78.73355)
				(xy 180.945076 78.337291) (xy 180.98112 78.189119) (xy 181.003239 77.99405) (xy 180.990215 77.836737)
				(xy 180.963134 77.723408) (xy 180.926098 77.612296) (xy 180.920859 76.87227)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.SilkS")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.0754)
			(thermal_bridge_width 0.0754)
		)
		(polygon
			(pts
				(xy 180.818386 81.627936) (xy 180.32258 81.629005) (xy 180.32258 81.193696) (xy 180.445777 81.165093)
				(xy 180.641964 81.105429) (xy 180.818386 81.034636)
			)
		)
	)
	(embedded_fonts no)
)
